# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title:****TD 07** **Urban furniture for a cycle park p 1 /…**

**Publication reference: IPA ADRION 368/ No.7 (No.** **05-1091/3)**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments onits proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specificationsrequired** | **3.**  **Specificationsoffered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| 1 | **Benches –Клупи (30)**  Production and installation of benches made of high-quality materials: construction - Iron, 4 cm thick..) and backrest and seat made of wood suitable for public areas, painted with paints with high durability to outdoor conditions at the choice of the municipality with dimensions 150/45 cm, 150 cm length and 45 cm width - freestanding with backrest  Изработка и монтажа на **клупи за седење** изработени од висококвалитетни материјали:конструкција-Железо, со дебелина од 4 цм..) и наслон и седиште изработено од дрво погодно за јавни површини, бојадисани со бои со висока издржливост на надворешни услови по избор на општината со димензии 150/45 см , 150 см должина и 45 см ширина- самостојни со наслон |  |  |  |
| 2 | **Garbage cans – канти за ѓубре (10)**  Purchase and installation of external garbage cans volume: 28 l, dimensions (l / w / h) mm: 400/350/900 on a single holder, steel column - placed on a foundation in the ground 30/30/30 cm MB 20, material characteristics of the cans: made of sheet metal with a thickness of 0.8 mm) with an enamel varnish finish with the possibility of choosing a colour  Набавка и поставување на надворешни канти за ѓубре обем: 28 л, димензии (д/ш/в)мм: 400/350/900 на единечен држач, челично столбче- поставено на темел во земја 30/30/30 см МБ 20, карактеристики на материјалот на кантите:изработени од лим со дебелина 0,8 мм)со финиш емајл лак со можност за избор на боја |  |  |  |
| 3 | Road signs – патокази Production, transport and installation of road signs - Production and installation of road signs - 30cm x 50 cm, tin, white with text written in black in Macedonian and English.  Изработка, транспорт и монтажа на патокази-Изработка и поставување на патокази - 30cm x 50 cm, лимени, бели со текст испишан со црна боја на македонски и англиски јазик |  |  |  |