# GRB

# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title:** Supply of **TD 02 – Supply of Van for transportation of disadvantage people p 1 /…**

**Publication reference:**IPA ADRION 368/ No.2 (No.05-96/2)

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments onits proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Van for transportation of disadvantage people**  Vehicle should have the capacity to transport at least two people in wheel chairs at the same time and be equipped with a hydraulic lift with a load capacity of at least 180 kg.  Type of engine -Diesel; Fuel emission: Euro E6.  **Seats minimum: 1 driver + 8 passengers + 2 people ina wheelchair; Doors 2 front, 1 side, 1 rear bifold; Air conditioning in the vehicle in the front in the driver's compartment and in the back in the passenger compartment**  **Airbag for the driver; Electric headlight adjustment; Trip computer; Tinted glasses**  **Side windows on both sides of the vehicle**  **Automatic locking of the vehicle when starting**  **Safety belts on all seats with force limitationtightening; Parking sensors; Roof fan**  **Movable ladder for easier entry of passengers placed on the right slidedoor**  **Lighting of the interior space**  **2 places for accommodating people in manual wheelchairs**  **Electric regulation of front windows**  **Central locking of the doors with remote control**  **Start&Stop system**  **Factory built-in radio with Bluetooth, USB and speakers**  **Radio commands of a steering wheel; Trip computer; Digital clock display; Scheduled service maintenance** |  |  |  |